{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["log"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"log","index":0,"n_rows":56,"n_cols":14,"rows_kept":56,"cut":false,"hidden":false,"merged":[[1,3,1,4],[1,5,1,6],[2,3,2,4],[2,5,2,6],[3,3,3,4],[3,5,3,6],[4,3,4,4],[4,5,4,6],[6,1,6,4],[6,5,6,9],[7,1,7,4],[7,5,7,9],[8,1,8,4],[8,5,8,9],[9,1,9,4],[9,5,9,9],[10,1,10,4],[10,5,10,9],[11,1,11,4],[11,5,11,9],[12,1,12,4],[12,5,12,9],[13,1,13,4],[13,5,13,10],[21,0,21,13],[22,1,22,3],[22,4,22,10],[26,1,26,3],[26,4,26,10],[25,1,25,3],[24,1,24,3],[24,4,24,10],[25,4,25,10],[23,1,23,3],[23,4,23,10],[27,1,27,3],[27,4,27,10],[28,1,28,3],[28,4,28,10],[29,1,29,3],[29,4,29,10],[30,1,30,3],[30,4,30,10],[31,1,31,3],[31,4,31,10],[32,1,32,3],[32,4,32,10],[33,1,33,3],[33,4,33,10],[34,1,34,3],[34,4,34,10],[35,1,35,3],[35,4,35,10],[36,1,36,3],[36,4,36,10],[37,1,37,3],[37,4,37,10],[38,1,38,3],[38,4,38,10],[39,1,39,3],[39,4,39,10],[40,1,40,3],[40,4,40,10],[41,1,41,3],[41,4,41,10],[42,1,42,3],[42,4,42,10],[43,1,43,3],[43,4,43,10],[44,1,44,3],[44,4,44,10],[45,1,45,3],[45,4,45,10],[46,1,46,3],[46,4,46,10],[52,0,52,13],[55,1,55,3],[55,4,55,10],[56,1,56,3],[56,4,56,10],[57,1,57,3],[57,4,57,10],[58,1,58,3],[58,4,58,10],[59,1,59,3],[59,4,59,10],[60,1,60,3],[60,4,60,10],[61,1,61,3],[61,4,61,10],[62,1,62,3],[62,4,62,10],[63,1,63,3],[63,4,63,10],[64,1,64,3],[64,4,64,10],[65,1,65,3],[65,4,65,10],[66,1,66,3],[66,4,66,10]]}
[]
[null,"决议人","决议","签名",null,"日期"]
[null,"测试执行",null,null,null,"2021-09-17"]
[null,"测试审核"]
[null,"批准"]
[]
[null,"版本定义描述",null,null,null,"主线版本（优化细节）",{"$nulls":4},"是\n否更新"]
[null,"兼容产品",null,null,null,"XC6X0芯片系列"]
[null,"SDK版本号",null,null,null,"xc6x0_sdk_4.03",{"$nulls":4},"Y"]
[null,"此次更新相关demo",null,null,null,"GPIO_TIMER_ADC_Demo",{"$nulls":4},"Y"]
[null,"BLE协议栈库更新",{"$nulls":8},"Y"]
[null,"脱机烧录软件版本号",null,null,null,"V2.02"]
[null,"更新日期",null,null,null,"2021-09-17"]
[null,"是否归档",null,null,null,"是"]
{"$rows_empty":7}
["1. 当前版本新增/修改 功能（在母版本内容基础上添加，即：先复制母版本的内容过来，后面添加本次的，本次的以红色字体显示）"]
[null,"功能模块名称",null,null,"功能/BUG 描述",{"$nulls":6},"版本号","测试时间","测试审核"]
[null,"gpadc",null,null,"增加ADC 校准接口， 优化ADC demo（优化去抖、0通道无法采集的bug）",{"$nulls":6},"sdk_4.03","2021-09-17","符合设计"]
[null,"Sleep",null,null,"深睡例程，增加唤醒后读取RTC时间的功能",{"$nulls":6},"sdk_4.02","2021-09-07","符合设计"]
[null,"gpadc",null,null,"优化GADC采集，提升采集速度，稳定性 解决切换频道FIFO数值与通道对应不上的概率性问题。",{"$nulls":6},"sdk_4.02","2021-09-07","符合设计"]
[null,"Sleep",null,null,"1、优化下降沿唤醒偶尔出现唤醒失败问题(RTC_Handler中增加延时解决)\n2、深睡将FLASH 设置为powerdown模式，可以优化8.3ua电流",{"$nulls":6},"sdk_4.01","2021-04-25","符合设计"]
[null,"gpadc",null,null,"1、gpadc 选择 AVDD（3V3）做为参考电压的代码及注释\n2、将校准ADC精度寄存器操作加入demo里",{"$nulls":6},"sdk_4.01","2021-04-25","符合设计"]
[null,"HIDdemo",null,null,"优化HIDdemo",{"$nulls":6},"sdk_4.01","2021-04-25","符合设计"]
[null,"TouChuan_Demo",null,null,"修改蓝牙透传发包方式为分包发送",{"$nulls":6},"sdk_4.01","2021-04-25","符合设计"]
[null,"脱机烧录程序",null,null,"脱机烧录器上电开机增加检测sram 串口缓冲区数组 坏点 生成的offlin.bin的固件",{"$nulls":6},"V2.01","2021-04-25","符合设计"]
[null,"添加OTA_demo",null,null,"APP采用透传 app设置mtu为270个字节、 连接间隔调到最快， ble支持OTA",{"$nulls":6},"sdk_4.01","2021-04-25","符合设计"]
[null,"20210513 优化睡眠",null,null,"优化深度睡眠和浅睡眠",{"$nulls":6},"sdk_4.01","2021-04-25","符合设计"]
{"$rows_empty":19}
["2.bug严重程度简介（归档用）"]
[]
[]
[null,"功能模块名称",null,null,"功能/BUG 描述",{"$nulls":6},"版本号","测试执行","测试审核"]